**Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Employee # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Date \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Score \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Directions:**

Read each question and choose the best answer. There is only one correct answer for each question.

1. Individuals entering the Tankhouse without proper training are required to:
   1. Be accompanied by a qualified individual
   2. Sign in at the control room
   3. Review the hazard awareness checklist
   4. All the above
2. Which PPE item listed below is a minimum requirement to enter the Tankhouse?
   1. Respirator
   2. Goggles
   3. Long sleeves
   4. Cut resistant gloves
3. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ boots are required when working around suspended loads.
4. Forklifts in the Tankhouse will sound the horn when:
   1. Passing through a doorway
   2. Moving forward
   3. Around pedestrians
   4. Both a and c
5. Forklifts need to meet the chocking policy except when being used to harvest.
   1. True
   2. False
6. How long do you flush eyes or skin when contact with electrolyte?
   1. 5-10 minutes
   2. 15-20 minutes
   3. 30 minutes
   4. It is not necessary
7. What training is required in addition to Tankhouse Safety Certification to access above or below the cell line?
   1. Hot Work
   2. Overhead crane
   3. Tankhouse Electrical Safety
   4. Counter Balance Forklift
8. When performing any work with starter sheet material, cathodes, and banding you are required to wear:
   1. Green suit
   2. Cut resistant gloves
   3. PAPR
   4. Rubber boots
9. What gas is released when a cell becomes depleted of copper?
   1. Hydrogen
   2. Carbon Dioxide
   3. Hydrogen Sulfide
   4. Nitrogen
10. Grating should be inspected:
    1. At the end of shift
    2. When you have time
    3. By the supervisor
    4. During your workplace examination
11. When working with lead your work area must be cleaned up:
    1. When there is time
    2. By the next shift
    3. As work with lead is complete
    4. Only when MSHA is present
12. All lead contaminated PPE needs to be disposed of in the lead recycle bin not in the regular trash.
    1. True
    2. False